Filter:

Submit Search

# Compatibility of SMC/SNS firewalls

The SMC server manages SNS firewalls from version 4.3 upwards.

This table recaps the lowest versions of SNS firewalls required in order to be compatible with the following SMC features:

Feature/Object | Version of SMC | Lowest version of SNS firewall required
--- | --- | ---
Managing network interfaces (in read-only mode) | 3.0 | 3.7.0 1 As of SMC version 3.6, compatibility with 3.x versions of SNS will no longer be tested.
Managing network interfaces (in write mode) | 3.0.1 | 4.2.3
Managing “Diffusion Restreinte (DR)" mode | 3.1 | 4.3.21 LTSB or 4.7
Active Update distribution point | 3.1 | 4.3.3
Various versions of IKE supported on the same firewall | 3.1.3 | 3.7.0
Managing routing (in read-only mode) | 3.2 | 3.7.0
Routing (in write mode) | 3.2 | 4.2.3
SD-WAN support | 3.2 | 4.3.3
Managing IPSec virtual tunnel interfaces (VTI) | 3.4 | 4.2.3
Web services filtering | 3.4 | 4.4
QoS configuration | 3.6 | 4.3.15 LTSB or 4.5.3
Managing BIRD v2 dynamic routing | 3.6 | 4.8.1

NOTE
To be able to monitor the status of VPN topologies containing SN firewalls in version 4.2 or higher, you need to use an SMC server in version 3.0 or higher.