Filter:

Submit Search

# Compatibility of SMC/SNS firewalls

The SMC server manages SNS firewalls from version 4.3 upwards.

This table recaps the lowest versions of SNS firewalls required in order to be compatible with the following SMC features:

Feature/Object | Version of SMC | Lowest version of SNS firewall required
--- | --- | ---
Managing network interfaces (in read-only mode) | 3.0 | 3.7.0 1 As of SMC version 3.6, compatibility with 3.x versions of SNS will no longer be tested.
Managing network interfaces (in write mode) | 3.0.1 | 4.2.3
Managing “Diffusion Restreinte (DR)" mode | 3.1 | 4.3.21 LTSB or 4.7
Active Update distribution point | 3.1 | 4.3.3
Various versions of IKE supported on the same firewall | 3.1.3 | 3.7.0
Managing routing (in read-only mode) | 3.2 | 3.7.0
Routing (in write mode) | 3.2 | 4.2.3
SD-WAN support | 3.2 | 4.3.3
Managing IPSec virtual tunnel interfaces (VTI) | 3.4 | 4.2.3 and versions below 5.1.0
3.9 | 5.1.0
Web services filtering | 3.4 | 4.4
QoS configuration | 3.6 | 4.3.15 LTSB or 4.5.3
Managing BIRD v2 dynamic routing | 3.6 | 4.8.1

NOTE
In order to deploy route-based VPN topologies or virtual IPsec interfaces (VTIs) on SNS firewalls in version 5.1.0 or higher, you need to use an SMC server in version 3.9 or higher. Refer to the Recommendations section in the Release notes prior to any update.