Filter:

Submit Search

# Defining IPsec VTIs on SNS firewalls

This step is necessary for firewalls with network configurations that SMC does not manage. For more information, see the section Configure network interfaces.

Connect to every firewall in your topology and manually create IPsec VTIs in Network > Virtual interfaces using the .csv configuration file downloaded from SMC.

Refer to the SNS User guide as well for more information on how to create IPsec VTIs.

If you want IPsec interfaces to be automatically created, the .csv file contains all the information required to write serverd commands.

In this case, the column vti_interface_name must be entered manually. The value of the interface name is in the format ipsecXX for firewalls in versions below 5.1.0, and vtiXX for version 5.1.0 and higher, where XX is an increment that depends on the number of interfaces already on the firewall.

Now follow the last step.