Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# Advanced configuration

## Traffic encryption

The possible encryption parameters are:

Do not encrypt | This will disable the field Accept only encrypted traffic and allow the following algorithms as well as the MPPE offered.
Accept only encrypted traffic and allow the following algorithms | Allows the connection only if the client encrypts data.
40-bit MPPE | Allows the use of the 40-bit MPPE encryption protocol.
56-bit MPPE | Allows the use of the 56-bit MPPE encryption protocol.
128-bit MPPE | Allows the use of the 128-bit MPPE encryption protocol.