Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# USERS

The user authentication service requires the creation of user accounts at the firewall level. To access the features of this module, you must first create or configure your LDAP base (see document Directory configuration or module Users > Directory configuration).

The accounts contain all the information relating to these users:

ID

- Name
- First name
- E-mail address (optional)
- Phone number (optional)
- Description (optional)

The Users screen consists of 2 parts:

- A banner showing the various options
- The list of CNs (or users) in the left column, accompanied by information about them in the right column.

These are the tables indicating the maximum number of users that can be authenticated simultaneously according to the model of your firewall:

SN range | SN160(W) | SN210(W) | SN310 | SN510 | SN710 | SN910
Max. no. of users | 15 | 30 | 50 | 100 | 200 | 500
SN range | SN2000 | SN2100 | SN3000 | SN3100 | SN6000 | SN6100
Max. no. of users | 1000 | 2000 | 2500 | 4000 | 15000 | 15000
SN range | SNi40 |  |  |  |  |
Max. no. of users | 100 |  |  |  |  |
EVA range | EVA1 | EVA2 | EVA3 | EVA4 | EVAU |
Max. no. of users | 50 | 100 | 200 | 500 | 6000 |

To find out which characters are allowed or prohibited in various fields, please refer to the section Allowed names.