Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# IP

## “IPS” tab

### MTU

Impose MTU limit (force fragmentation) | MTU (Maximum Transmission Unit) represents the maximum size of an IP packet. If this option is selected, you will enable the next field and can define your limit.
Maximum MTU value | Define the maximum value of the IP datagram, between 140 and 65535 bytes.

### Fragmentation

Minimum fragment size (bytes) | The fragment has to be between 28 and 65535 bytes. The default value is 140 bytes.
Session will expire in (seconds) | This period has to be between 2 and 30 seconds.

NOTE

The IP protocol does not have a profile.