Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# General configuration

Enable PPTP server | Enables the configuration of the PPTP server on the firewall. This can be done by selecting the option Enable PPTP server.
IP addresses of PPTP clients (object) (mandatory) | Once the PPTP server has been enabled, a pool of private IP addresses must be created. The firewall will then assign available IP addresses from the pool to clients who connect in PPTP. A host group must be created, containing reserved addresses or an address range from the object database.

## Parameters sent to PPTP clients

DNS Server | The field DNS server allows sending the IP address of the DNS server to the client.
WINS server | The field WINS server allows sending the IP address of the WINS server to the client.

REMARK

The characters “_”, “-”, and “.” are allowed for PPTP user names