Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# General configuration tab

The General configuration tab allows the following parameters to be modified:

## General configuration

Refer to the section Allowed names to find out which characters are allowed and prohibited in various fields.

Firewall name | This name is used in alarm e-mails sent to the administrator and is displayed in the firewall’s main window. It can also be used as the DNS name of the captive portal if it was enabled and the option “Use firewall name or certificate CN as FQDN” was selected. The maximum supported length of the firewall name is 127 characters.
Firewall language (logs) | Choice of language, between French and English. This language is used for logs, syslog and the CLI configuration.
Keyboard (console) | Type of keyboard that the firewall supports. Five layouts are available: English, French, Italian, Polish or Swiss.

## Cryptographic settings

Enable regular retrieval of certificate revocation lists (CRL) | If this option is selected, the firewall will regularly check the validity of each CRL downloaded from the distribution points specified in the PKI. When a CRL is close to its expiry date or has expired, an alarm will then be generated.
Enable “ANSSI Diffusion Restreinte (DR)” mode | This option forces the firewall to abide by the ANSSI’s (French national information security agency) guidelines on the use of coprocessors and cryptographic accelerators on products under evaluation for qualification. It is an imperative on networks that fall under the “Restricted” classification. This mode relies in particular on the use of software versions for asymmetric and symmetric cryptographic algorithms and random key generation algorithms. As for symmetric encryption algorithms, "AES-NI" instructions available on certain products are exempt as they are made up only of “simple acceleration instructions” of certain cryptographic operations. When “ANSSI Diffusion Restreinte (DR)" mode is enabled from version 3.6.0 onwards, the following will occur: IPsec: the module will check whether the firewall is using version 2 of the IKE protocol. If this is not the case, a warning will appear, prompting the administrator to change the IPsec configuration. IPsec: the module will check whether the encryption algorithms used belong to DH19 and DH28 groups (ECP 256 and ECP Brainpool 256). If this is not the case, a warning will appear, prompting the administrator to change the IPsec configuration. IPsec: the module will check whether the encryption algorithm used is AES_GCM_16 (associated by default with SHA256 authentication). On firewalls equipped with Intel processors, the “ANSSI Diffusion Restreinte (DR)" mode will impose the use of the coprocessor's cryptographic hardware instruction sets. On firewalls equipped with other types of processors, the “ANSSI Diffusion Restreinte (DR)" mode will force such instruction sets to be disabled, causing performance to slow down during encryption. The “ANSSI Diffusion Restreinte (DR)" mode restricts the encryption suites that can be used on the authentication portal and on SSL VPN: only AES, SHA256, SHA384 and GCM encryption suites are allowed. Do note as well that the firewall must be rebooted in order to enable the “ANSSI Diffusion Restreinte (DR)” mode.

## Password policy

The indicated parameters will apply to all passwords and pre-shred keys defined on the firewall (VPN PPTP, IPsec VPN, internal LDAP directory, etc.). The parameters are:

Minimum password length | Indicate the minimum number of characters required for each password defined on the firewall. NOTE The value defined by default is 1 for the purpose of compatibility in the event existing configurations are migrated to version 2.
Mandatory character types | Select the mandatory types of characters to be included in each password: None: the password is not required to contain any alphanumeric or special characters, Alphanumeric: the password must contain at least an alphabetical character and a number, Alphabetical and special: the password must contain at least an alphanumeric character and a special character (‘#’, ‘@’, etc.)

NOTE
Refer to the section Allowed names to find out which characters are allowed and prohibited in various fields.

## Date/Time settings

Date | Firewall’s date. Select the date from the calendar. This field will be grayed out if NTP configuration has been enabled.
Time | Firewall’s time. This field will be grayed out if NTP configuration has been enabled.
Synchronize with your machine | By clicking on this button, the firewall will synchronize its time with your computer’s time. This field will be grayed out if NTP configuration has been enabled.
Time zone | Time zone defined for the firewall (GMT by default). The firewall has to be restarted if the time zone is changed.
Synchronize firewall time (NTP) | NTP (Network Time Protocol) is a protocol that makes it possible to synchronize the local clock on your computers with a time reference via your network. If this option is selected, your firewall will automatically be synchronized with the local time.

NOTE
The date and time set on your Stormshield Network firewall are important: they allow you to locate events in the log files. They are also useful in scheduling configurations.

### List of NTP servers

This table will only be accessible if you have selected the option Synchronize firewall time (NTP). If you have not done so, the list of NTP servers will be grayed out.

NTP servers (host or group-address range) (max 15) | The NTP server represents the remote clock with which your firewall will be synchronized. You can Add or Delete servers by clicking on the relevant buttons. When you click on Add, a new line will be added to the list of NTP servers. You may select an object from the drop-down list or create one by clicking on . It will then be possible to create a host, an IP address range or a group. Click on Apply after you have entered the data for the new object. NOTE NTP requests go through the default interface of the firewall. The interface used can be customized by adding the NTP server through the CLI / Serverd command "CONFIG NTP SERVER ADD". For more information on the syntax of this command, refer to the CLI Serverd Commands Reference Guide.
Password (ASCII) | Even though this is optional, you can enter a password for your NTP server which you can use for authentication.

## Advanced properties

### Hardware

The option for monitoring hardware activity Watchdog is available on all physical "S" model firewalls in the U Series.

Other firewalls in the U Series can benefit from this tool, which can improve troubleshooting and help. This mechanism is implemented by default but has to be enabled via the BIOS system. Please refer to the technical support department’s Knowledge Base for the full procedure.

Hardware monitoring timeout (watchdog) | This device tests the activity of the firewall’s system. The frequency of tests is defined by this timeout. When the system is idle, this watchdog will reboot the firewall and raise a system event (24). To stop monitoring, select Disable.

### Captive portal

Redirect to the captive portal | This option allows you to choose the name of the firewall used when generating URIs that redirect to the captive portal. There are four possible values: Use firewall's IP address. Use firewall's name. This refers to the name indicated in the Firewall name field in the General configuration section or the firewall's serial number if no name has been specified in this field Use the captive portal's certificate. This refers to the name of the firewall specified in the portal's certificate. Specify a domain name (FQDN).
Domain name (FQDN) | Enter a fully qualified DNS name for the firewall (e.g.: firewall.company.org). This field is only accessible when the "Specify a domain name (FQDN)" value was selected in the Redirect to the captive portal field.

## Industrial firewalls only (SNi40 models)

To ensure service continuity in an industrial setting, SNi40 model firewalls are equipped with a hardware bypass function, which when enabled, allows network traffic to pass through without being analyzed.

Do note that:

- This mechanism cannot be enabled on firewalls in a high availability configuration,
- This mechanism can only be enabled on the first two interfaces of the firewall.

Two of the firewall's operating modes are available:

- Security mode: this mode prioritizes network security and protection. The bypass mechanism cannot be enabled. This is the firewall's default operating mode.
- Safety mode: this mode prioritizes service continuity. The bypass mechanism will be enabled whenever the appliance breaks down or there is a power outage.

Whenever Safety mode is enabled, one of three types of bypass may be activated:

- SystemOff bypass: it will be activated when the appliance experiences an electrical failure or when there is a power outage.
- JustOn bypass: it will be activated when the appliance is restarted and will then be disabled.
- OnTimer bypass: when the product has to handle too many connections, this bypass will be activated after a period defined in the configuration of Safety mode. Once the bypass is activated, the firewall administrator can then reset Safety mode.

IMPORTANT
The proper operation of network traffic must be verified immediately after a manual reset. The firewall will not recognize connections initiated during the active bypass phase and will systematically reject them.

When bypass is activated, the first two interfaces of the firewall will be represented as follows:

Enable safety mode | When this option is selected, you will be enabling the firewall's bypass mechanism. All three activation modes will be automatically available.
Safety mode timeout | Select the period after which the OnTimer bypass must be activated. The various possible values are: 1 min 1 min 30 sec 2 min 2 min 30 sec 3 min 3 min 30 sec 4 min
Reset safety mode | When the OnTimer bypass is activated, you can click on this button in order to disable it and return the firewall to safety mode.