Filter:

Submit Search

# Disabling Diffusion Restreinte mode on SMC and firewalls

The super administrator (admin account) can disable DR mode on the SMC server. Disabling DR mode from SMC does not disable it on firewalls.

To disable DR mode:

1. Go to Maintenance > SMC Server > Settings tab > “ANSSI Diffusion Restreinte (DR)" mode.
2. Disable "ANSSI Diffusion Restreinte (DR)" mode.
   DR mode is disabled on the SMC server. This operation does not make any changes to firewalls, which can continue to connect to the SMC server.