Filter:

Submit Search

# Installing a new connecting package on an SNS firewall

When an SNS firewall is already connected to SMC, and you wish to replace the connecting package, proceed as follows. This procedure applies to SNS in version 5.1.0 and upwards.

Ensure in advance that there are no configuration deployments, SNS CLI script runs or SMC updates in progress.

1. In SMC, generate a new connecting package from the firewall's System > Configuration menu.

2. On the firewall, run the command CLI CONFIG RESTORE list=fwadmin,network < /tmp/my_file.pack by providing the package (.pack).