Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# Antivirus tab

## POP3 protocol

Contents of the e-mail | This field allows modifying the text of the message received when a virus is detected in an e-mail. Example: Your Stormshield Network firewall has detected a virus in this e-mail - the embedded antivirus has cleaned it; infected attachments were removed.

## SMTP protocol

SMTP error code | Restricted to 3 digits, this field allows defining the error code that the SMTP server will receive when a virus is detected in a sent e-mail. Example: 554
Accompanying message | This field contains the message that will be sent to the SMTP server when a virus is detected. Example: 5.7.1 Virus detected.

## FTP protocol

FTP error code | Restricted to 3 digits, this field contains the error code that the user or the FTP server will receive when a virus is detected in a transferred file. Example: 425
Accompanying message | This spot is reserved for the message that will be sent with the error code when a virus is detected while sending/receiving a file to/from an FTP server. Example: Virus detected. Transfer aborted.