Filter:

Submit Search

IMPORTANT
SNS 3.x versions have reached End of Maintenance since July 1st, 2024.
We recommend that you update your SNS firewalls to a version with maintenance to guarantee the protection of your infrastructure.

# Configuration tab

## System disk

You are currently using this partition | Your firewall’s system disk is divided into two partitions, which allow you to back up your data. This section indicates the partition on which the product started up.
Main partition | Version of the firmware installed on the main partition.
Backup partition | Version of the firmware installed on the backup partition.
Upon startup, use the | Choose the partition on which you wish to start the appliance: the main or backup partition. Main partition: if this option is selected, your firewall will use this partition at startup. Backup partition: represents the last partition that you backed up. If this option is selected, your firewall will use this partition at startup.
Back up the active partition | This button allows you to back up the active partition (the one indicated by You are currently using this partition) on the other partition.

## Maintenance

Reboot the firewall | Click on this button to restart your firewall directly.
Shut down the firewall | Click on this button if you wish to shut down your firewall.

## High availability

Make a firewall stay active | In the event both firewalls in your HA cluster are in an active state or start up at the same time, this option allows designating a member that will have priority in staying active. NOTE Before defining a remote firewall as the firewall with priority, check that your firewalls are synchronized. This is important as modifications made to the current configuration on the firewall would be lost during the switch.

## System report (sysinfo)

Download the system report | This button allows you to obtain various types of information about your firewall in sysinfo format. Using this feature, you will be able to find out, for example, the model of the firewall, its serial number, its current status and the status of its memory, etc.